(C) SAF Tehnika JS

* Introduction
* Aranet PRO/PRO Plus/PRO Plus LTE Firmware upgrade
* Firmware upgrading instructions
* Troubleshooting

******************************
Introduction

Thank you for purchasing and using Aranet base station!
All Aranet PRO/PRO Plus/PRO Plus LTE base stations include embedded local webserver Aranet SensorHUB. Easy to use interface allows viewing, analyzing, and comparing data in real time, setting thresholds for alarms as well as exporting reports.
Responsive design of the software adapts to smartphone, tablet, or laptop.

******************************
Firmware upgrade

To ensure a better stability and getting all enhancements manufacturer recommends upgrading Aranet base staion embedded software (firmware) to the latest available version.
The latest available for download firmware file can be found on https://aranet.com/downloads.

******************************
Firmware upgrading can be completed semi-automatically from the WebGUI or Aranet Cloud or manually.

Semi-automatic upgrading instructions from WebGUI (the base station must be connected to internet):
1. Login into Aranet base station WebGUI as user having Administrator rights.
2. Navigate to the SYSTEM menu FIRMWARE tab.
    If a newer firmware version is available for downloading, press the INSTALL button and follow the on-screen instructions.

Semi-automatic upgrading instructions from Aranet Cloud (the base station must be connected to internet and registered to Aranet Cloud):
1. Login into Aranet Cloud as user having Administrator rights.
2. Navigate to the BASE STATIONS menu.
    The base station needing the firmware upgrade will be indicated.
3. Press MANAGE button, and after establishing the connection click on FIRMWARE.
4. Follow the on-screen instructions.

Manual firmware upgrading instructions:
1. Download the firmware zip packed archive file at https://aranet.com/downloads to your computer.
2. Unpack zip archive to the folder you are able to access. Zip achvive contains:
    - Firmware file named "AranetProUpgrade-vX.Y.Z.tar.gz"
    - This README.txt file
    Don't change file name!
3. Turn On Aranet base and wait for system to load.
4. Login into Aranet base WebGUI as user having Administrator rights.
5. Navigate to SYSTEM menu and select FIRMWARE tab.
6. Click on CHOOSE FIRMWARE FILE button.
7. In the opened window find the folder where you unpacked the firmware file, select this file and click "Open" button.
8. Enter Administrator password when asked and press OK.
9. File uploading process will start.
10. When uploading and installing process is finished, notificating message is displayed and device reboots.
11. Wait about 2 minutes and reload browser window.
12. Navigate to SYSTEM menu, FIRMWARE tab and check firmware version.

*****************************
Troubleshooting

If firmware upgrade fails, check the firmware file name and extention:
    - File name must be "AranetProUpgrade-vX.Y.Z", where X.Y.Z is the version number;
    - File extension must be ".tar.gz".
Some archivator software tends to unpack all available archive levels of the file. Switch off this archiver's feature to leave archived .gz file untouched.
For example, MacOS users should deselect "Keep expanding if possible" feature of built-in archivator.

If nothing helps, contact support@aranet.com.

*****************************

v4.11.15 changelog
    Aranet Cloud
        * Data upload optimization
    Integrations
        * BACnet IP stability improvement

*****************************

v4.11.9 changelog
    Sensors
        * Weight sum virtual sensor reintroduced
    Integrations
        * MQTT - Weight sum virtual sensor support
        * Bacnet, InfluxDB - "Sensor ID" and "Sensor Type" fields added

*****************************

v4.10.12 changelog
    Integrations:
        * Modbus TCP/IP - fixed address offsets for the metrics, new fields
        * Notification delays affects all integrations alarms

*****************************

v4.9.9 changelog
    Sensors
        * Aranet Light Spectrum sensor support
    Graph
        * Save manual graph min/max limits in URL rather than browser local storage
    Aranet Cloud
        Cloud management
        * Implemented remote reboot
        * Implemented remote developer diagnostics file download

*****************************

v4.8.4 changelog
    Integrations:
        * Modbus TCP/IP -  added Discrete Input registers for measurement threshold alarm states
        * MQTT - Application-Layer Protocol Negotiation support

*****************************

v4.7.19 changelog
    System:
        * Added network and Aranet Cloud status indicators to toolbar
    Integrations:
        * InfluxDB v2 support
    Aranet Cloud:
        * Management license support

*****************************

v4.7.15 changelog
    Aranet Cloud:
        * Base provisioning credential generation fix

*****************************

v4.7.12 changelog
    Integrations:
        * BACnet - Measurement unit ID hotfix

*****************************

v4.7.2 changelog
    Sensors:
        * Radon Plus Pro support
    System:
        * Korean region support
    Integrations:
        * MQTT Last Will and Testament (LWT) messaging support

*****************************
v4.6.4 changelog
    Sensors:
        * 4xT-probe sensor support
        * T/RH Mini support
        * Terralink transmitter support
    Integrations:
        * MQTT (Sensor Management) delete process now has additional topics: "pending" and "status"
        * Fixed sensor data reception delay when low on free storage space
    Networking:
        * LTE connection stability improvement

*****************************
v4.5.3 changelog
    Integrations:
        * Modbus - added option to change Unit ID (or Device ID)
        * Modbus - additional field "address" added for the measurement object in auto-generated registry mapping file
        * BACnet - added option to filter inbound requests by using IP address filter

    Aranet Cloud:
        * Cloud connected base station functionality added

*****************************
v4.4.4 changelog
    New feature:
        * Pulse counter conversion offset - possibility to input the current meter value to apply an offset to the converted value
    Improvements:
        * Minor changes in BACnet EDE file content

*****************************
v4.3.9 changelog:
    Integrations:
        * Removed unnecessary reinitialization for BACnet server on Failover script execution
        * BACnet fix for missing measurements
        * BACnet fix for battCharge replacement with battery
    Networking:
        * Fix network failover to reduce LTE traffic
    webGUI:
        * Fix for DIAGNOSTICS data download on base station without Internet connection

*****************************
v4.3.7 changelog:
    Integrations:
        * Fix Modbus colliding sensor offset re-assignment in the auto-generated layout file. Non-existing sensors are now removed from the file.
        * Fix Modbus auto-generated layout file address overwrite correction for existing sensors
    Networking:
        * Fix network failover when Ethernet is disconnected

*****************************
v4.3.2 changelog:
    Integrations:
        * Modbus auto-generated JSON file now contains sensor "name" and "group name" info
        * MQTT integration compatibility with Azure Event Grid
    Networking:
        * Added network interface failover in case of lost connectivity
    LTE:
        * Blocked SIM PIN recovery with PUK code added


*****************************
v4.2.5 changelog:
    Integrations:
        * Derived measurement dimension and unit configuration is passed to all Integrations cache and updated on user-initiated sensor configuration changes
        * MQTT "name" field issue eliminated
    LTE (Aranet PRO Plus LTE base only):
        * Modem management improvement
    webGUI:
        * Few User Interface pages esthetics change

Known issue:
    ! Internet connection is not switching to LTE automatically when existing WiFi or Ethernet configured connection drops.

*****************************
v4.1.3 changelog:
    Cloud base management:
        * Support remote sensor pairing from Aranet Cloud
        * Support license management from Aranet Cloud
        * Block web UI while management session is active
    MQTT:
        * Allow leading forward-slash ("/") in root topic
    Licenses:
        * License slots increased from 5 to 10
        * The integration license's timer is paused when integration is disabled

Known issue:
    ! Internet connection is not switching to LTE automatically when existing WiFi or Ethernet configured connection drops.

*****************************
v4.0.2 changelog:
    Soil moisture sensors:
        * Use improved Hilhorst pore water electric conductivity preset by default for newly paired sensors.
    LTE:
        * Roaming support
        * Improved stability
    BACnet:
        * After the system boots, the 'Reliability' property for measurement objects is set to 'Communication failure' until measurements have been received.

Known issue:
    ! Internet connection is not switching to LTE automatically when existing WiFi or Ethernet configured connection drops.

*****************************
v4.0.0 changelog:
    Cloud base management
        * Firmware update initiation from Aranet Cloud

Known issue:
    ! Internet connection is not switching to LTE automatically when existing WiFi or Ethernet configured connection drops.

*****************************